#

##

##

##

##

##

##

    猩ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.14.2
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Cortex-M0 sonix Flex license: MDK-ARM Standard Cortex-M only: 12 user(s) (mdk_cm_std) Borrow:

    Tool Versions:
    Toolchain:       MDK-ARM Standard Cortex-M only: 12 user(s)  Version: 5.11.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.04
    Assembler:       Armasm.exe V5.04
    Linker/Locator:  ArmLink.exe V5.04
    Library Manager: ArmAr.exe V5.04
    Hex Converter:   FromElf.exe V5.04
    CPU DLL:         SARMCM3.DLL V5.11.0.0
    Dialog DLL:      DARMCM1.DLL V1.11.00.0
    Target DLL:      SNLink\SNLINK.dll V1.0.0.2
    Dialog DLL:      TARMCM1.DLL V1.08.00.0

    Project:
    D:\新人訓練\Open Short\Open_Short_FW\TW\SNLED2735\20200922\SNLED2735_I2C_Demo Code V1.03_20200922\SNLED2735_SN32F248B_DemoCode_V1_03.uvprojx
    Project File Date:  09/23/2020

    Output:
    *** Using Compiler 'V5.04', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'SNLED2735_DemoCode'
    compiling main.c...
    compiling LED_Function.c...
    compiling LED_Effect.c...
    compiling I2C0.c...
    compiling usbdesc.c...
    compiling usbepfunc.c...
    compiling usbhw.c...
    compiling usbram.c...
    compiling usbuser.c...
    compiling hidram.c...
    compiling hiduser.c...
    compiling Utility.c...
    assembling startup_SN32F240B.s...
    compiling system_SN32F240B.c...
    linking...
    Program Size: Code=9410 RO-data=23366 RW-data=80 ZI-data=1184
    FromELF: creating hex file...
    After Build - User command #2: HexConvert.exe SN32F240B "D:\新人訓練\Open Short\Open_Short_FW\TW\SNLED2735\20200922\SNLED2735_I2C_Demo Code V1.03_20200922\obj\SN32F240B.HEX" 0
    INI_Ver = V29
    EXE_Ver = V20
    CheckSum = 0x8242
    ".\obj\SN32F240B.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.1.0.pack
                    ARM::CMSIS:CORE:3.30.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 3.30.0

    Package Vendor: SONiX
                    http://liveupdate.sonix.com.tw/sonix/develop_tool/MCU/DFP/SONiX.SN32F2_DFP.1.3.2.pack
                    SONiX::Device:Startup:1.1.1
                    SONiX SN32F2 Series Device Support and Examples
       * Component: Startup Version: 1.1.1

    Collection of Component include folders:
      D:\新人訓練\Open Short\Open_Short_FW\TW\SNLED2735\20200922\SNLED2735_I2C_Demo Code V1.03_20200922\RTE
      C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.1.0\CMSIS\Include
      C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:3.30.0
          Source file:   CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c

       * Component: SONiX::Device:Startup:1.1.1
          Source file:   Device\Source\system_SN32F240B.c
          Source file:   Device\Source\ARM\startup_SN32F240B.s