***********************************************************************************************************
*                                                                                                         *
*        SONiX 8-Bit MCU Development Tool Readme                                                          *  
*                                                                                                         *
***********************************************************************************************************
***********************************************************************************************************
    SONiX IDE                  M2IDE_V149  <M2IDE_V149.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm149    <M2Asm149.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 04/06/2019
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8F2267F,SZK671F,SN8P27184

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A, 	SN8P2977,
    SN8P2977A,	SN8F29E49,  SN8P2988,	SN8F2267F,  SZK671F,	SN8P27184
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm148>

1. Support new chip:
   SN8F2267F, SZK671F, SN8P27184

2. Update file:
   SN8P2988.inc, SN8P2977A.inc, ChipInfo.ini

***********************************************************************************************************
*                                                                                                         *
*        SONiX 8-Bit MCU Development Tool Readme                                                          *  
*                                                                                                         *
***********************************************************************************************************
***********************************************************************************************************
    SONiX IDE                  M2IDE_V148  <M2IDE_V148.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm148    <M2Asm148.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 15/01/2019
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2988

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A, 	SN8P2977,
    SN8P2977A,	SN8F29E49,  SN8P2988
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm148>

1. Support new chip:
   SN8P2988

2. Update file:
   ChipInfo.ini
***********************************************************************************************************
    SONiX IDE                  M2IDE_V147  <M2IDE_V147.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm147    <M2Asm147.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 29/05/2018
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8F29E49

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A, 	SN8P2977,
    SN8P2977A,	SN8F29E49
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm147>

1. Support new chip:
   SN8F29E49

2. Update inc file chip:
   SN8P2977A, SN8P2977

3. Update bit file chip:
   SN8P2977A

4. Update bol file chip:
   SN8P2977A

5. Update file:
   ApprovedFormGenerator.exe
***********************************************************************************************************
    SONiX IDE                  M2IDE_V146  <M2IDE_V146.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm146    <M2Asm146.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 26/02/2018
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2977A

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A, 	SN8P2977,
    SN8P2977A
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm146>

1. Support new chip:
   SN8P2977A


***********************************************************************************************************
    SONiX IDE                  M2IDE_V145  <M2IDE_V145.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm145    <M2Asm145.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 16/01/2017
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2977

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A, 	SN8P2977
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm145>

1. Support new chip:
   SN8P2977

2. Update inc file chip:
   SN8P29E39, SN8P2947, SN8P2967

3. Update file:
   Sn8AFGen.ini

***********************************************************************************************************
    SONiX IDE                  M2IDE_V144  <M2IDE_V144.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm144    <M2Asm144.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 29/04/2016
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    NA

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm144>

1. Support new chip:
   NA

2. Update inc file chip:
   NA

3. Update file:
   NA

***********************************************************************************************************
    SONiX IDE                  M2IDE_V143  <M2IDE_V143.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm143    <M2Asm143.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 14/04/2016
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    NA

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm143>

1. Support new chip:
   NA

2. Update inc file chip:
   SN8PC22,SN8PC20,SN8P26L38,SN8P26L34,SN8P2511,SN8P2623,SN8P2723,SN8F25E21L,SN8F25E24L,SN8F25E25,SN8F25E25L,
   SN8F26E61,SN8F26E61L,SN8F26E64L,SN8F26E65,SN8F26E65L,SN8F26E611L,SN8F27E61,SN8F27E61L,SN8F27E62L,SN8F27E64L,
   SN8F27E65,SN8F27E65L,SN8F27E611L,SN8FMD21L,SN8FMD22L,SN8FMD23L,SN8FMD24L,SN8FMD25,SN8FMD25L,SN8P2501D,SN8F29E39

3. Update file:
   ChipInfo.ini(add SN8F27E63L)

***********************************************************************************************************
    SONiX IDE                  M2IDE_V142  <M2IDE_V142.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm142    <M2Asm142.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 31/12/2015
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2267E, SZK671A

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611,  SN8P2267E,  SZK671A
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm142>

1. Support new chip:
   SN8P2267E, SZK671A

2. Update inc file chip:
   NA
   
3. Update bit file chip:
   SN8P2761
   
4. Update function:
   ApprovedFormGenerator.exe

***********************************************************************************************************
    SONiX IDE                  M2IDE_V141  <M2IDE_V141.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm141    <M2Asm141.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 07/08/2015
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2761, SN8P2962, SN8P27611

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967,   SN8P2761,   SN8P2962,   SN8P27611
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm141>

1. Support new chip:
   SN8P2761, SN8P2962, SN8P27611

2. Update inc file chip:
   SN8PC21A, SN8P27L11B, SN8P2949, SN8P2929, SN8F22E88B, SN8F29E39, SN8P2967
   
3. Update bit file chip:
   SN8P2929, SN8P2839, SN8P2967, SN8P2501B
   
4. Update function:
   ApprovedFormGenerator.exe

***********************************************************************************************************
    SONiX IDE                  M2IDE_V140  <M2IDE_V140.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm140    <M2Asm140.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 01/08/2015
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8F29E39,  SN8F29E38,  SN8F22E88B,  SN8P27L11B, SN8PC21A, SN8F22E87B, SN8F22E84B, SN8F22E83B,
    SN8F2967

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A, SN8P25221,  SN8P25223,  SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F29E39,  SN8F29E38,  SN8F22E88B, SN8P27L11B, SN8PC21A  , SN8F22E87B, SN8F22E84B,
    SN8F22E83B, SN8F2967
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm140>

1. Support new chip:
   SN8F29E39,  SN8F29E38,  SN8F22E88B,  SN8P27L11B, SN8PC21A, SN8F22E87B, SN8F22E84B, SN8F22E83B,
   SN8F2967

2. Update inc file chip:
   SN8F27E23,  SN8P25L31,  SN8P22421
   
3. Update bit file chip:
   SN8P2524,  SN8P2929,  SN8P2949
   
4. Update function:
   ApprovedFormGenerator.exe

5. Remove chip:
   SN8F27E23L

***********************************************************************************************************
    SONiX IDE                  M2IDE_V139  <M2IDE_V139.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm139    <M2Asm139.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 06/20/2014
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P25113E, SN8F2722A,  SN8P2501D,  SN8F22831,   SN8P2741A,  SN8F25E21,   SN8F25E21L, SN8P25L31,
    SN8F27E63L, SN8PNB168,  SN8P25117,  SN8P27113B,  SN8P27113A, SN8P27124,   SN8P27226A, SN8P27227A,
    SN8P27231,  SN8P27232,  SN8F26E681, SN8F26E681L, SN8P27411A, SN8P27412A,  SN8P25221,  SN8P25223,
    SN8P25232,  SN8P25233,  SN8F27E23,  SN8F27E23L

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,
    SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L,  SN8FMD22,
    SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,
    SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,
    SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,  SN8P25113E, SN8F2722A,
    SN8P2501D,  SN8F22831,  SN8P2741A,  SN8F25E21,  SN8F25E21L, SN8P25L31,  SN8F27E63L, SN8PNB168,
    SN8P25117,  SN8P27113B, SN8P27113A, SN8P27124,  SN8P27226A, SN8P27227A, SN8P27231,  SN8P27232,  
    SN8F26E681, SN8F26E681L,SN8P27411A, SN8P27412A,  SN8P25221,  SN8P25223, SN8P25232,  SN8P25233,
    SN8F27E23,  SN8F27E23L
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm139>

1. Support new chip :
   SN8P25113E, SN8F2722A,  SN8P2501D,  SN8F22831,   SN8P2741A,  SN8F25E21,   SN8F25E21L, SN8P25L31,
   SN8F27E63L, SN8PNB168,  SN8P25117,  SN8P27113B,  SN8P27113A, SN8P27124,   SN8P27226A, SN8P27227A,
   SN8P27231,  SN8P27232,  SN8F26E681, SN8F26E681L, SN8P27411A, SN8P27412A,  SN8P25221,  SN8P25223,
   SN8P25232,  SN8P25233,  SN8F27E23,  SN8F27E23L

2. Bug Fixed chip:
   NA

3. Update inc file chip:
   SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL,  SN8F25E24L,  SN8F25E25L, SN8F25E27L, SN8F25E28L,
   SN8F26E61L, SN8F26E64L, SN8F26E65L,  SN8F26E67L, SN8F26E68L,  SN8F26E611L,SN8F27E61L, SN8F27E62L,
   SN8F27E64L, SN8F27E65L, SN8F27E611L, SN8FMD21L,  SN8FMD22L,   SN8FMD23L,  SN8FMD24AL, SN8FMD24L,
   SN8FMD25AL, SN8FMD25L
   
4. Support new function :
   NA
   
5. Remove function :
   NA
   
6. Update bol file chip:
   SN8FMD25A  
 
7. Update bit file chip:
   SN8P2949

8. Remove chip :
   SN8P27122

***********************************************************************************************************
    SONiX IDE                  M2IDE_V138  <M2IDE_V138.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm138    <M2Asm138.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 10/18/2013
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,  SN8F26E67,  SN8F26E67L,  SN8F26E68,  SN8F26E68L,
    SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,   SN8FMD24A,  SN8FMD24AL,  SN8FMD25A,  SN8FMD25AL,  
    SN8P25234,  SN8F2267D,

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L,
    SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L, 
    SN8FMD22,   SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B,  SN8F25E27,  SN8F25E27L, SN8F25E28,
    SN8F25E28L, SN8F26E67,  SN8F26E67L, SN8F26E68,  SN8F26E68L, SN8P2623,   SN8P2723,   SN8P2929,
    SN8FMD25A,  SN8FMD24A,  SN8FMD24AL, SN8FMD25A,  SN8FMD25AL, SN8P25234,  SN8F2267D,
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm138>

1. Support new chip :
   SN8F25E27,  SN8F25E27L, SN8F25E28,  SN8F25E28L,  SN8F26E67,  SN8F26E67L,  SN8F26E68,  SN8F26E68L,
   SN8P2623,   SN8P2723,   SN8P2929,   SN8FMD25A,   SN8FMD24A,  SN8FMD24AL,  SN8FMD25A,  SN8FMD25AL,
   SN8P25234,  SN8F2267D,

2. Bug Fixed chip:
   NA  

3. Update inc file chip:
   SN8F2255,  SN8F2255B,  SN8F2288,  SN8P2213,  SN8P2236,  SN8P2267C,  SN8P2501C,  SN8P2711A,  SN8P2711B,
   SN8P2712,  SN8P2949,   SN8P22421
   
4. Support new function :
   SN8P2839_Macro.h
   
5. Remove function :
   2949_Macro.h
   
6. Update bol file chip:
   NA    
 
7. Update bit file chip:
   SN8P2318,  SN8P2501B,  SN8P2511,  SN8P2523,  SN8P2602C,  SN8P2839,  SN8P2929,  SN8P2949
***********************************************************************************************************
    SONiX IDE                  M2IDE_V137  <M2IDE_V137.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm137    <M2Asm137.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Date: 08/20/2012
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    NA      

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L,
    SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L, 
    SN8FMD22,   SN8FMD22L,  SN8FMD23,   SN8FMD23L,  SN8P2711B
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm137>

1. Support new chip :
   NA    

2. Bug Fixed chip:
   NA  

3. Update inc file chip:
   NA
   
4. Support new function :
   NA
   
5. Remove function :
   MPIII Writer    
   
6. Update bol file chip:
   NA     
***********************************************************************************************************
    SONiX IDE                  M2IDE_V136  <M2IDE_V136.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm136    <M2Asm136.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    MP-III Writer PC Software  V1.14       <MPIII_WtV114.exe>
    Date: 07/12/2012
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2711B      

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L,
    SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L, SN8FMD21,   SN8FMD21L, 
    SN8FMD22,   SN8FMD22L,  SN8FMD23,   SN8FMD23L
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm136>

1. Support new chip :
   SN8P2711B    

2. Bug Fixed chip:
   SN8PC22  

3. Update inc file chip:
   SN8P2204,   SN8P2213,   SN8P2236,   SN8P22421,   SN8P2267,   SN8P2267C
   SN8F2255,   SN8F2255B,  SN8F22721,  SN8F22721B,  SN8F2288,   SN8F25E25  
   SN8F26E61,  SN8F27E61,  SN8F26E65,  SN8F27E65,   SN8F27E93,  SN8FMD25
   SZK671
   
4. Support new function :
   Live Update
   
5. Remove function :
   NA     
   
6. Update bol file chip:
   NA     

<MP-III Writer PC Software V1.14>

1. Update Drv. 
   All series MCU

2. Add new chip :
   SN8P2711B     
***********************************************************************************************************
    SONiX IDE                  M2IDE_V135  <M2IDE_V135.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm135    <M2Asm135.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    MP-III Writer PC Software  V1.13       <MPIII_WtV113.exe>
    Date: 06/08/2012
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8FMD21,   SN8FMD21L,  SN8FMD22,   SN8FMD22L,  SN8FMD23,   SN8FMD23L   

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411,  SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2,   
    SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L,
    SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  SN8F25E25L 
    
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm135>

1. Support new chip :
   SN8FMD21,   SN8FMD21L,  SN8FMD22,   SN8FMD22L,  SN8FMD23,   SN8FMD23L    

2. Bug Fixed chip:
   NA  

3. Update inc file chip:
   SN8P2947,   SN8P2949,  SN8P2267C,   SZK671,  SN8FMD25,   SN8F25E25,  SN8P2511,   SN8F26E65   
   
4. Support new function :
   NA
   
5. Remove function :
   NA     
   
6. Update bol file chip:
   NA     

<MP-III Writer PC Software V1.13>

1. Update Drv. 
   All series MCU

2. Add new chip :
   SN8FMD21,   SN8FMD21L,  SN8FMD22,   SN8FMD22L,  SN8FMD23,   SN8FMD23L    
***********************************************************************************************************
    SONiX IDE                  M2IDE_V134  <M2IDE_V134.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm134    <M2Asm134.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    MP-III Writer PC Software  V1.12       <MPIII_WtV112.exe>
    Date: 04/17/2012
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2, SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,
    SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, 
    SN8F25E25,  SN8F25E25L

    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411   
         
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm134>

1. Support new chip :
   SN8P2267C,  SZK671,     SN8P2949,   SN8P2711A2, SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,
   SN8FMD25,   SN8FMD25L,  SN8F26E64,  SN8F26E64L, SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, 
   SN8F25E25,  SN8F25E25L     

2. Bug Fixed chip:
   NA  

3. Update inc file chip:
   SN8P2501B1   
   
4. Support new function :
   NA
   
5. Remove function :
   SN8P2267B     
   
6. Update bol file chip:
   NA     

<MP-III Writer PC Software V1.12>

1. Update Drv. 
   All series MCU

2. Add new chip :
   SN8P2711A2, SN8P27122,  SN8P2511,   SN8FMD24,   SN8FMD24L,  SN8FMD25,   SN8FMD25L,
   SN8F26E64,  SN8F26E64L, SN8F26E65,  SN8F26E65L, SN8F25E24,  SN8F25E24L, SN8F25E25,  
   SN8F25E25L    
***********************************************************************************************************
    SONiX IDE                  M2IDE_V133  <M2IDE_V133.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm133    <M2Asm133.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    MP-III Writer PC Software  V1.11       <MPIII_WtV111.exe>
    Date: 02/15/2012
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    NA        	
    
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947,   SN8PC2014, 
    SN8PC2016,  SN8P2704B,  SN8P2524,   SN8P27411   
         
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm133>

1. Support new chip :
   NA     

2. Bug Fixed chip:
   NA  

3. Update inc file chip:
   SN8P2839   
   
4. Support new function :
   NA
   
5. Remove function :
   NA     
   
6. Update bol file chip:
   NA     

<MP-III Writer PC Software V1.11>

1. Update Drv. 
   All series MCU
    
***********************************************************************************************************
    SONiX IDE                  M2IDE_V132  <M2IDE_V132.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm132    <M2Asm132.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    MP-III Writer PC Software  V1.10       <MPIII_WtV110.exe>
    Date: 02/02/2012
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8PC2014, SN8PC2016, SN8P2704B, SN8P2524, SN8P27411        	
    
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L,SN8P2267B, 	SN8P2839,   SN8P2947
         
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm132>

1. Support new chip :
   SN8PC2014, SN8PC2016, SN8P2704B, SN8P2524, SN8P27411     

2. Bug Fixed chip:
   NA  

3. Update inc file chip:
   SN8P2947   
   
4. Support new function :
   NA
   
5. Remove function :
   NA     
   
6. Update bol file chip:
   SN8P2947     

<MP-III Writer PC Software V1.10>

1. Update Drv. 
   All series MCU

2. Update Flash_MP.IAP    
***********************************************************************************************************
    SONiX IDE                  M2IDE_V131  <M2IDE_V131.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm131    <M2Asm131.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    MP-III Writer PC Software  V1.09       <MPIII_WtV109.exe>
    Date: 09/05/2011
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8P2267B, SN8P2839, SN8P2947       	
    
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L,  	   
    SN8F26E611, SN8F26E611L,SN8F27E611, SN8F27E611L 
         
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm131>

1. Support new chip :
   SN8P2267B,   SN8P2839,   SN8P2947    

2. Bug Fixed chip:
   SN8P2236,   SN8P2318,   SN8P2712,   SN8PC20  

3. Update inc file chip:
   SN8P2501B1,   SN8P26L34,   SN8P26L38
   
4. Support new function :
   a.  Approved Form Generator
   
5. Remove function :
   a.  Easy Writer
   b.  MP Writer
   c.  Gang Writer     
   
6. Update USB Driver, support for Win7 64-bit version of the Windows operating system    

<MP-III Writer PC Software V1.09>

1. Update Drv. 
   SN8F26E00,   SN8F27E00 series MCU Drv.
***********************************************************************************************************
    SONiX IDE                  M2IDE_V130  <M2IDE_V130.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm130    <M2Asm130.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.09       <MPIII_WtV109.exe>
    Date: 05/23/2011
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip :
    SN8F26E611, SN8F26E611L, SN8F27E611, SN8F27E611L       	
    
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L, SN8P25231,  SN8PC22,    SN8F26E61,  SN8F26E61L, SN8F27E61,  SN8F27E61L  	   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm130>

1. Support new chip :
   SN8F26E611, SN8F26E611L, SN8F27E611, SN8F27E611L   

2. Bug Fixed chip:
   SN8P2735,   SN8P2743 

3. Update inc file chip:
   SN8P2318,   SN8P2604A,   SN8P2712,   SN8P2758,   SN8F26E61,   SN8F27E61 

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.09>

1. Add new chip :
   SN8F26E611, SN8F26E611L, SN8F27E611, SN8F27E611L 

2. Update Drv. 
   SN8P26L31,   SN8P26L32,   SN8P26L321,   SN8P26L34,   SN8P26L37,   SN8P26L38,   SN8PC20,   SN8P2267
   SN8F2251,    SN8F22511,   SN8F22521,    SN8F2253,    SN8F22531,   SN8F2255,    SN8F2251B, SN8F22511B
   SN8F22521B,  SN8F2253B,   SN8F22531B,   SN8F2255B,   SN8F2271,    SN8F22711,   SN8F22721, SN8F2277
   SN8F2271B,   SN8F22711B,  SN8F22721B,   SN8F2277B,   SN8F2283,    SN8F2288,    SN8F27E62, SN8F27E62L	
   SN8F27E64,   SN8F27E64L,  SN8F27E65,    SN8F27E65L,  SN8F26E61,   SN8F26E61L,  SN8F27E61, SN8F27E61L
***********************************************************************************************************
    SONiX IDE                  M2IDE_V129  <M2IDE_V129.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm129    <M2Asm129.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.09       <MPIII_WtV109.exe>
    Date: 01/21/2011
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P25231,   SN8PC22,   SN8F26E61, SN8F26E61L, SN8F27E61,  SN8F27E61L       	
 
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523,   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, 
    SN8F27E94,  SN8F27E94L 	   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm129>

1. Support new chip :
   SN8P25231,   SN8PC22,   SN8F26E61, SN8F26E61L, SN8F27E61,  SN8F27E61L   

2. Bug Fixed : Chip SN8P2743   

3. Bug Fixed : Chip SN8P2522

4. Bug Fixed : Chip SN8P2523  

5. Update SN8P2758 inc file

6. Update SN8F27E65 inc file

7. Update SN8P2501C inc file 

8. Update SN8P22421 inc file
 
9. Update SN8P2602C inc file

10. Update SN8P2602C1 inc file

11. Update SN8F27E93 inc file 

12. Update SN8P2522 inc file

13. Update SN8P2523 inc file
    
<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.09>

1. Add new chip :
   SN8P25231,   SN8F26E61, SN8F26E61L, SN8F27E61,  SN8F27E61L 

2. Update Drv. 

3. Remove Read EEPROM function 

4. Operation mode after unplug usb cable
***********************************************************************************************************
    SONiX IDE                  M2IDE_V128  <M2IDE_V128.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm128    <M2Asm128.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.08       <MPIII_WtV108.exe>
    Date: 09/01/2010
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, SN8F27E94,  SN8F27E94L       	
 
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712,   SN8P2523 	   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm128>

1. Support new chip :
   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, SN8F27E94,  SN8F27E94L   

2. Add SN8P2501C bit file for SN8ICE 2K

3. Update SN8P2242 bit file  
   (a) P1.7 input mode issue (pin status always low)

4. Update SN8P2722 bit file   
   (a) TC0M value changed by single step at the PCL = 0x00DA 

5. Update SN8F2255B bit file  
   (a) Single step function fail after setting a breakpoint at the PCH = 0x04,PCL = 0xCE 

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.08>

1. Add new chip :
   SN8P2241,   SN8P2317,   SN8P2602C1, SN8P2711A1, SN8F27E93,  SN8F27E93L, SN8F27E94,  SN8F27E94L

2. Update Drv. (Program function modified to Program + Verify function for on-line and off-line) 
***********************************************************************************************************
    SONiX IDE                  M2IDE_V127  <M2IDE_V127.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm127    <M2Asm127.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 07/01/2010
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2523	
      
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743,   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,
    SN8P2712	   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm127>

1. Support new chip :
   SN8P2523  

2. Bug Fixed : Chip SN8P2712
   (a) ADM issue   

3. Bug Fixed : Chip SN8P2318
   (a) P2M issue 
	       
4. Update inc files 
   (a) Add GreenMode, SleepMode, SlowMode, Slow2Normal macro 

5. Update SN8F22721B, SN8P2242 bit files  
   (a) Single step function fail after setting a breakpoint at the PCL = 0xCE 

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Add new chip :
   SN8P2523

***********************************************************************************************************
    SONiX IDE                  M2IDE_V126  <M2IDE_V126.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm126    <M2Asm126.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 05/28/2010
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,  SN8P2712	
      
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L, SN8P2742,   SN8P2743	   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm126>

1. Support new chip :
   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,  SN8P2712  

2. Bug Fixed : Chip SN8P2522
	       (a)  P56 IO mode direction issue   

3. Bug Fixed : Chip SN8P2743
	       (a)  Can't setting BZM register issue

4. Bug Fixed : Chip SN8P2715
	       (a)  ADC function issue 
	       
5. Bug Fixed : SN8ICE2K
	       (a)  Can't use Easy Writer function
	       
6. Update macro3.h file for @JMP_A macro

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Add new chip :
   SN8P2318,   SN8P2501B1, SN8P2501C,  SN8P2602C,  SN8P2712   

2. Update Drv. 
   SN8P2501B,  SN8F2271B, SN8F22711B,  SN8F22721B, SN8F2277B  
***********************************************************************************************************
    SONiX IDE                  M2IDE_V125  <M2IDE_V125.exe>
    SONiX IDE for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII, Embedded ICE
    Assembler and Debugger     M2Asm125    <M2Asm125.exe> 
    Assembler and Debugger for SN8P2XXX, SN8FXXXX Family
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 02/11/2010
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2742,   SN8P2743	
      
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21,    SN8P2233,   SN8P2242,					
    SN8P22421,  SN8P2521,   SN8P26L37,  SN8P2708B,  SN8F27E62,  SN8F27E62L, SN8F27E64,  SN8F27E64L,
    SN8F27E65,  SN8F27E65L   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm125>

1. Support new chip :
   SN8P2742,   SN8P2743  

2. Add SN8A2617.bit file for SN8ICE 2K PlusII

3. Update USB Driver, support for 64-bit version of the Windows operating system 

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Add new chip :
   SN8P2742,   SN8P2743  

2. Update Drv. 
   SN8PC20,    SN8P26L31,   SN8P26L32,   SN8P26L321,   SN8P26L34,   SN8P26L37,   SN8P26L38,   SN8F2251,
   SN8F2253,   SN8F2255,    SN8F22511,   SN8F22521,    SN8F22531,   SN8F2251B,   SN8F2253B,   SN8F2255B,  
   SN8F22511B, SN8F22521B,  SN8F22531B,  SN8F22721,    SN8F2271,    SN8F2277,    SN8F22711,   SN8F2271B,
   SN8F2277B,  SN8F22711B,  SN8F22721B,  SN8F2288,     SN8F27E62,   SN8F27E62L,  SN8F27E64,   SN8F27E64L,
   SN8F27E65,  SN8F27E65L	      
***********************************************************************************************************
    SONiX IDE                  M2IDE_V124  <M2IDE_V124.exe>   (for SN8ICE 2K, SN8ICE 2K Plus, SN8ICE 2K PlusII)
    Assembler and Debugger     M2Asm124    <M2Asm124.exe>     (Only for SN8P2XXX Family)
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 01/06/2010
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2267,   SN8PC21	
      
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,   SN8P2267,   SN8PC21							
       
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm124>

1. Support new chip :
         SN8P2233,   SN8P2242,   SN8P22421,   SN8P2521,   SN8P26L37,   SN8P2708B,
         SN8F27E62, SN8F27E62L,  SN8F27E64,   SN8F27E64L, SN8F27E65,   SN8F27E65L   	

2. Bug Fixed : Chip SN8P2308
	       (a) green mode wakeup issue 

3. Bug Fixed : Chip SN8P2213
	       (a) USB enumeration process failure 
	       
4. Bug Fixed : Chip SN8F2288
	       (a)  stack data has random fail issue  

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Add new chip :
	 SN8P2233,   SN8P2242,   SN8P22421,   SN8P2521,   SN8P26L37,   SN8P2708B,
   SN8F27E62, SN8F27E62L,  SN8F27E64,   SN8F27E64L, SN8F27E65,   SN8F27E65L

2. Update Drv.     
***********************************************************************************************************
    SONiX IDE                  M2IDE_V123  <M2IDE_V123.exe>         (Only for SN8ICE 2K)
    Assembler and Debugger     M2Asm123    <M2Asm123.exe>           (Only for SN8P2XXX Family)
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 01/06/2010
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2267,   SN8PC21	
      
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2735,   SN8P2754,   SN8P2755,   SN8P2758,   SN8F2251,	
    SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,  SN8F22531,  SN8F2251B,  SN8F2253B,  SN8F2255B,  
    SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  
    SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288					
       
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm123>

1. Support new chip :
         SN8P2267,  SN8PC21	

2. Bug Fixed : Chip SN8F2288
	       (a) stack bug 

3. Bug Fixed : Chip SN8P26L34
	       (a) green mode wake up function with RTC bug for SN8ICE2K
	       
3. Bug Fixed : Chip SN8P2722
	       (a) register A have changed after execute NOP instruction       	            

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Add new chip :
	 SN8P2267, SN8PC21 Drv. 
***********************************************************************************************************
    SONiX IDE                  M2IDE_V122  <M2IDE_V122.exe>         (Only for SN8ICE 2K)
    Assembler and Debugger     M2Asm122    <M2Asm122.exe>           (Only for SN8P2XXX Family)
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 09/07/2009
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip :
    SN8P2732,   SN8P2733,   SN8P2734,   SN8P2754,   SN8P2755	
      
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2735,  	SN8P2758,   SN8F2251,   SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,	SN8F22531,
    SN8F2251B,  SN8F2253B,  SN8F2255B,  SN8F22511B, SN8F22521B, SN8F22531B,	SN8F22721,	SN8F2271, 
    SN8F2277,   SN8F22711,  SN8F2271B,  SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288,		
       
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm122>

1. Support new chip :
         SN8P2732, SN8P2733, SN8P2734, SN8P2754, SN8P2755	

2. Bug Fixed : Chip SN8F2288
	       (a) Timer bug
	       (b) stack bug (for address 0x108e)

3. Fixed install USB Driver fail bug       

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Add new chip :
	 SN8P2732,	SN8P2733, SN8P2734, SN8P2754, SN8P2755 Drv. 
***********************************************************************************************************
    SONiX IDE                  M2IDE_V121  <M2IDE_V121.exe>         (Only for SN8ICE 2K)
    Assembler and Debugger     M2Asm121    <M2Asm121.exe>           (Only for SN8P2XXX Family)
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.07       <MPIII_WtV107.exe>
    Date: 07/29/2009
***********************************************************************************************************

<A> Supporting Chip:
	
    Support fully function emulation of following chips:
    SN8P2501A,	SN8P2602A,  SN8P2604,   SN8P2606,   SN8P2608,   SN8P270XA,  SN8P2711,   SN8P2714,
    SN8P27142, 	SN8P27143,  SN8P2715,   SN8P2308,   SN8P26042,  SN8P2612,   SN8P2613,   SN8P2624,
    SN8P2603A, 	SN8P2611,   SN8P2622,   SN8P2501B,  SN8P2602B,  SN8PC13,    SN8P2201,   SN8P2202,
    SN8P2203,  	SN8P2204,   SN8A2617,   SN8P2604A,  SN8P2614,   SN8P2808,   SN8P2212,   SN8P2213,
    SN8P22121, 	SN8P26L32,  SN8P26L321, SN8P26L34,  SN8P2722,   SN8P2807,   SN8P2234,   SN8P2236,
    SN8P2238,  	SN8P2711A,  SN8P26L38,  SN8PC20,    SN8P26042A, SN8P22021,  SN8P26L31,  SN8P2522,
    SN8P2735,  	SN8P2758,   SN8F2251,   SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,	SN8F22531,
    SN8F2251B,  SN8F2253B,  SN8F2255B,  SN8F22511B, SN8F22521B, SN8F22531B, SN8F22721,  SN8F2271, 
    SN8F2277,   SN8F22711,  SN8F2271B,  SN8F2277B,  SN8F22711B, SN8F22721B, SN8F2288   
        
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm121>

1. Modify SN8P2522, SN8P2735, SN8P2758, SN8PC20 INC file. 

2. Bug Fixed : Chip SN8P2213
	       (a) Can't clear T0IRQ and TC0IRQ
	       
3. Bug Fixed : Chip SN8P2522
	       (a) Timer bug   
	       
4. Bug Fixed : Chip SN8F2288
	       (a) Timer bug 	          

5. Add MPIII Writer function Link at File Toolbar       

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.07>

1. Update IAP  

2. Update Drv.
    SN8F2251,   SN8F2253,   SN8F2255,   SN8F22511,  SN8F22521,	SN8F22531,
    SN8F2251B,  SN8F2253B,  SN8F2255B,  SN8F22511B, SN8F22521B, SN8F22531B, 
    SN8F22721,  SN8F2271,   SN8F2277,   SN8F22711,  SN8F2271B,  SN8F2277B, 
    SN8F22711B, SN8F22721B, SN8F2288 
***********************************************************************************************************
    SONiX IDE                  M2IDE_V120  <M2IDE_V120.exe>         (Only for SN8ICE 2K)
    Assembler and Debugger     M2Asm120    <M2Asm120.exe>           (Only for SN8P2XXX Family)
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.06       <MPIII_WtV106.exe>
    Date: 04/30/2009
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip SN8F2277, SN8F22711, SN8F2251B, SN8F2253B, SN8F2255B, SN8F22511B
	 									 SN8F22521B, SN8F22531B, SN8F2271B, SN8F2277B, SN8F22711B, SN8F22721B
			
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238,  SN8P2711A, SN8P26L38, SN8PC20, SN8F2251, SN8F2253, SN8F2255, SN8F22511, 
    SN8F22521, SN8F22531, SN8P26042A, SN8F22721, SN8F2271, SN8P22021, SN8P26L31, SN8P2522, 
    SN8P2735,  SN8P2758 ,SN8F2288. 
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm120>

1. Add new chip SN8F2277, SN8F22711, SN8F2251B, SN8F2253B, SN8F2255B,
	 SN8F22511B, SN8F22521B, SN8F22531B, SN8F2271B, SN8F2277B, SN8F22711B, SN8F22721B function.
	  
2. Modify SN8P2522, SN8P2735, SN8P2758 INC file. 

3. Bug Fixed : Chip SN8F2288
	       (a) When setting P1OC[2] = 1,pGPIO5[0] status will become open drain type
	       (b) P1M[0],P1M[1] Can't read 
	       (c) P1M[0],P1M[1] can't use bset and bclr instructions  

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.06>

1. Add new chip SN8F2277, SN8F22711, SN8F2251B, SN8F2253B, SN8F2255B,
	 SN8F22511B, SN8F22521B, SN8F22531B, SN8F2271B, SN8F2277B, SN8F22711B, SN8F22721B Drv. 

2. Update Drv.  
***********************************************************************************************************
    SONiX IDE                  M2IDE_V119  <M2IDE_V119.exe>         (Only for SN8ICE 2K)
    Assembler and Debugger     M2Asm119    <M2Asm119.exe>           (Only for SN8P2XXX Family)
    Easy Writer PC Software    V2.08
    MP Writer PC Software      V1.09       <MP_WtV109.exe>
    Gang Writer PC Software    V1.02       <Gang_WtV102.exe>
    MP-III Writer PC Software  V1.06       <MPIII_WtV106.exe>
    Date: 01/19/2009
***********************************************************************************************************

<A> Supporting Chip:
	
    Support new chip SN8P2522, SN8P2735, SN8P2758 ,SN8F2288.
			
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238,  SN8P2711A, SN8P26L38, SN8PC20, SN8F2251, SN8F2253, SN8F2255, SN8F22511, 
    SN8F22521, SN8F22531, SN8P26042A, SN8F22721, SN8F2271, SN8P22021, SN8P26L31. 
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm119>

1. Add new chip SN8P2522, SN8P2735, SN8P2758 ,SN8F2288 function.

2. Add check ICE Hardware type.

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.06>

1. Add new chip SN8P2522, SN8P2735, SN8P2758 ,SN8F2288 Drv. 

***********************************************************************************************************
        SONiX IDE               	M2IDE_V118	<M2IDE_V118.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger 	 	M2Asm118	<M2Asm118.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software   	V2.08
	MP Writer PC Software		V1.09	        <MP_WtV109.exe>
	Gang Writer PC Software		V1.02   	<Gang_WtV102.exe>
	MP-III Writer PC Software  	V1.06		<MPIII_WtV106.exe>
	Date: 11/13/2008
***********************************************************************************************************

<A> Supporting Chip:

    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238,  SN8P2711A, SN8P26L38, SN8PC20, SN8F2251, SN8F2253, SN8F2255, SN8F22511, 
    SN8F22521, SN8F22531, SN8P26042A, SN8F22721, SN8F2271, SN8P22021, SN8P26L31. 
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm118>

1. Bug Fixed : Chip SN8P26L38
	       (a) Setting bank2 and bank3 RAM Value¡Athe value not to show IDE UI
	       (b) P4.0 ~ P4.3 pull-up function fail   

2. Bug Fixed : Chip SN8P2614
	       (a) When the EXT_32K is selected in code option,to simulate can achieve RTC function,
		   but can not wake up the system from Green Mode.	

3. Modify SN8F2250, SN8F2270 INC file.

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

No Change.

<Gang Writer PC Software V1.02>

No Change.

<MP-III Writer PC Software V1.06>

1. Update Drv. 
  
***********************************************************************************************************
        SONiX IDE               	M2IDE_V117	<M2IDE_V117.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger 	 	M2Asm117	<M2Asm117.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software   	V2.08
	MP Writer PC Software		V1.09	        <MP_WtV109.exe>
	Gang Writer PC Software		V1.02   	<Gang_WtV102.exe>
	MP-III Writer PC Software  	V1.06		<MPIII_WtV106.exe>
	Date: 07/18/2008
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8F22721, SN8F2271, SN8P22021, SN8P26L31.
 
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238,  SN8P2711A, SN8P26L38, SN8PC20, SN8F2251, SN8F2253, SN8F2255, 
    SN8F22511, SN8F22521, SN8F22531, SN8P26042A. 
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm117>

1. Add SN8F22721, SN8F2271, SN8P22021, SN8P26L31 chip function.

2. Remove SN8P2735 chip function.

3. Bug Fixed : Fix the problem of the abnormal WDT overflow time for Chip SN8P2230.

4. Bug Fixed : Under High_Clk  = IHRC_8M and Fcpu = Fosc/1, the ICE emulation of SN8P26L3X's 
	       Sleep_MODE will arise the program counter's disorder after waken up.  

5. Bug Fixed : Chip SN8P2722
	       (a) Under set the TC0 timer as PWM mode and select the CLK source as external input from P0.0, 
	           the P0.0's clock signal will be interfered by any change to FP00.
	       (b) T0 timer can not wake up the system from Green Mode.
	       (c) When the XTAL_32K is selected in code option, the system can not look up the table with the MOVC instruction.  			

6. Modify SN8P2604A ,SN8PC13 INC file.

<Easy Writer PC Software V2.08>

No Change.

<MP Writer PC Software  V1.09>

1. Add Auto Install USB Driver function.

<Gang Writer PC Software V1.02>

1. Add Auto Install USB Driver function.

<MP-III Writer PC Software V1.06>

1. Add SN8F22721 ,SN8F2271 ,SN8P22021 ,SN8P26L31 Drv.

2. Remove SN8P2735 chip function.  

***********************************************************************************************************
        SONiX IDE               	M2IDE_V116	<M2IDE_V116.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger 	 	M2Asm116	<M2Asm116.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software   	V2.08
	MP Writer PC Software		V1.08	        <MP_WtV108.exe>
	Gang Writer PC Software		V1.01   	<Gang_WtV101.exe>
	MP-III Writer PC Software  	V1.05		<MPIII_WtV105.exe>
	Date: 04/24/2008
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8F2251, SN8F2253, SN8F2255, SN8F22511, SN8F22521, SN8F2231, SN8P26042A, SN8P26L31.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238,  SN8P2711A, SN8P2735, SN8P26L38, SN8PC20, SN8F2251, SN8F2253, SN8F2255, 
    SN8F22511, SN8F22521, SN8F22531, SN8P26042A. 
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm116>

1. Add SN8F2251, SN8F2253, SN8F2255, SN8F22511, SN8F22521, SN8F22531, SN8P26L31 and SN8P26042A chip function.

2. Bug Fixed : When using the approach of Project to develop the mode, if you open one ROM which has the 
	       bigger size chip with writing code.For example, if we assumed  the 4K ROM size has written 
               more than 2K's code,and we re-opened the one ROM size with the smaller chip to write the code. 
	       Just like the 2K ROM size has written the full code on 2K, to compile the result of code 
	       size was wrong calculation, it will be calculated by  last compile more than 2K's code size.

3.Bug Fixed : In Chip SN8P2808, if the system is in slow mode, the ROM code value fetched by the¡§movc¡¨instruction 
              will get wrong.

4. Add SN8P2708A "@RST_WDT" macro. 

<Easy Writer PC Software V2.08>

No Change.


<MP Writer PC Software  V1.08>

No Change.


<Gang Writer PC Software V1.01>

No Change.


<MP-III Writer PC Software V1.05>

1. Update .DRV file : To improve the anti-interference ability during IHRC calibration. 
2. Bug Fixed :  Security checksum calculate error of SN8P26L3X and SN8PC20.  

***********************************************************************************************************
        SONiX IDE               	M2IDE_V115	<M2IDE_V115.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm115	<M2Asm115.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.08
	MP Writer PC  Software		V1.08   	<MP_WtV108.exe>
	Gang Writer PC  Software	V1.01   	<Gang_WtV101.exe>
	MP-III Writer PC Software  	V1.04		<MPIII_WtV104.exe>
	Date: 01/08/2008
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2711A, SN8P2735, SN8P26L38, SN8PC20.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238,  SN8P2711A, SN8P2735, SN8P26L38, SN8PC20.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm115>

1. Bug Fixed : Chip SN8P2614 and SN8P2722 single step execute MOVC instruction is incorrect.

2. Revise Fcpu=Fosc/N Option of Code Option. Chip revised are S8KE_TEST, SN8P2708A, SN8P2602A,
   SN8A2617, SN8P2808, SN8P2715, SN8P2604A, SN8P2604, and SN8P2501A.

3. When Printer Port Address is unable to use, show error message that revises Printer Port Address of BIOS. 

4. Bug Fixed : Under Vista operating system, IDE is unable to install Printer Port Driver.

5. Add SN8P2711A, SN8P2735, SN8P26L38, and SN8PC20 chip function.

6. Support Security0 Code Option and Security1 Code Option. 

7. Add Green mode limiting conditions.

8. Support Operating mode control macro programs.


<Easy Writer PC Software V2.08>

No Change.


<MP Writer PC Software V1.08>

No Change.


<Gang Writer PC Software V1.01>

No Change.


<MP-III Writer PC Software V1.04>

1. Bug Fixed : MP-III Writer USB Driver is unable to install.

2. Update .DRV file : To IHRC body, revise IHRC checks mechanism.

3. Bug Fixed : While upgrading IAP, DRV, SN8 file, execute Auto Program, Program, Blank Check,
               Verify, Read function will cause USB fail.
   
4. Support Security0 Code Option and Security1 Code Option.


***********************************************************************************************************
        SONiX IDE               	M2IDE_V114	<M2IDE_V114.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm114	<M2Asm114.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.08
	MP Writer PC Software		V1.08   	<MP_WtV108.exe>
	Gang Writer PC Software		V1.01   	<Gang_WtV101.exe>
	MP-III Writer PC Software  	V1.03		<MPIII_WtV103.exe>
	Date: 09/06/2007
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2234, SN8P2236, SN8P2238.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807, SN8P2234, SN8P2236,
    SN8P2238.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm114>

1. Forbid Rolling Code range to contain ROM Code Address 0x00 and 0x08.

2. Rolling Code start address can only be in ROM Code odd address.

3. Rolling Code is the biggest can only establish 4 Word Length.

4. Bug Fixed : IDE will disable PC operating system 'Stand by' mode after initializing ICE.

5. IDE support SN8P2210 can be used on Full Speed USB MCU-V1.0 ICE and Full Speed USB MCU-V2.0 ICE.

6. Bug Fixed : When SN8P26L34 execute CALL instruction in ROM code address 0x1000 ~ 0x1FFB, will push wrong RET address
               (0x0001 ~ 0x0FFC) to stack. The correct RET address should be 0x1001 ~ 0x1FFC.

7. Add SN8P2234, SN8P2236, and SN8P2238 new chip function.

8. Bug Fixed : Sometimes SN8P2808 P0.0 external trigger can't wakeup ICE in green mode.


<Easy Writer PC Software V2.08>

1. Forbid Rolling Code to use selecting of "Highest Word is Low Address".

2. Forbid Rolling Code range to contain ROM Code Address 0x00 and 0x08.

3. Rolling Code start address can only be in ROM Code odd address.

4. Rolling Code is the biggest can only establish 4 Word Length.


<MP Writer PC Software V1.08>

1. Forbid Rolling Code to use selecting of "Highest Word is Low Address".

2. Forbid Rolling Code range to contain ROM Code Address 0x00 and 0x08.

3. Rolling Code start address can only be in ROM Code odd address.

4. Rolling Code is the biggest can only establish 4 Word Length.


<Gang Writer PC Software V1.01>

No Change.


<MP-III PC Software V1.03>

1. Forbid Rolling Code to use selecting of "Highest Word is Low Address".

2. Forbid Rolling Code range to contain ROM Code Address 0x00 and 0x08.

3. Rolling Code start address can only be in ROM Code odd address.

4. Rolling Code is the biggest can only establish 4 Word Length.

5. Update .DRV file : (1) When program fail, Writer will reprogram 4 times again.
                      (2) To IHRC body, increase IHRC Recheck mechanism.


***********************************************************************************************************
        SONiX IDE               	M2IDE_V113	<M2IDE_V113.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm113	<M2Asm113.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.07
	MP Writer PC Software		V1.07   	<MP_WtV107.exe>
	Gang Writer PC Software		V1.01   	<Gang_WtV101.exe>
	MP-III Writer PC Software  	V1.02		<MPIII_WtV102.exe>
	Date: 06/14/2007
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121, SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, SN8P2807.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm113>

1. Bug Fixed : After revises ROM code in ROM window of IDE, will update ROM code in the ICE. When execute ICE Reset,
               the ROM code in ROM window will be recovered, but ROM code in the ICE is not recovered.

2. Bug Fixed : While single step execute SN8P2708A and SN8PC13 chip function, watch dog overflow will happen.
               Free run will not happen.

3. Bug Fixed : Execute ADC function of SN8P2708A, the ADC value(ADB) sometimes is 0xFF.

4. Bug Fixed : The SN8PC13 and SN8P2613 program is unable to set I/O Port, but can be set by IDE window directly.

5. Bug Fixed : SN8P2604A I/O Port5 operation error.

6. Bug Fixed : SN8P2614 causes T0IRQ to be set as 1 that T0C.7 is changed 0 by 1, and it is unable to wake up by T0
               after entering Green mode.

7. Revise OTP Program Type = 12 Security Check Sum algorithm.

8. Add OTP Program Type = 13.

9. Add SN8P26L32, SN8P26L321, SN8P26L34, SN8P2722, and SN8P2807 chip function.

10. Update SN8P2213 inc file.


<Easy Writer PC Software V2.07>

No Change.


<MP Writer PC Software V1.07>

No Change.


<Gang Writer PC Software V1.01>

No Change.


<MP-III Writer PC Software V1.02>

1. Bug Fixed : The setting of Rolling Code will be altered after pressing OK key, for example
               If "Word Alignment" is "Lowest word is low address", and will be altered as "Highest word is low address"
               after pressing OK key.
               If "Rolling Method" is "No Use Rolling Code", and will be altered as "Auto-Inc from filename.INI" after
               pressing OK key.

2. Add show progress bar function while upgrading IAP and DRV.


***********************************************************************************************************
        SONiX IDE               	M2IDE_V112	<M2IDE_V112.exe>          (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm112	<M2Asm112.exe>            (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.07
	MP Writer PC Software		V1.07  	 	<MP_WtV107.exe>
	Gang Writer PC Software		V1.01   	<Gang_WtV101.exe>
	MP-III Writer PC Software  	V1.00		<MPIII_WtV100.exe>
	Date: 02/13/2007
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2614, SN8P2808, SN8P2212, SN8P2213, SN8P22121.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A, SN8P2614, SN8P2808, SN8P2212, SN8P2213,
    SN8P22121.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm112>

1. Bug Fixed : Will change RAM value when free run to RET instruction. Single step will not happen.

2. Bug Fixed : The 2-cycle instruction of write RAM (such as ADD/SUB/RLCM/RRCM ,etc.) will not execute when
               free run and stop at breakpoint of next instruction. Single step will not happen.

3. Add SN8P2614 chip function.

4. Add SN8P2808 chip function.

5. Remove SN8P2308 MUL instruction.

6. Add OTP Program Type 12 for SN8P26L32 and SN8P26L34.

7. Bug Fixed : When switch over to ROM window and close IDE, will unable normal operation of ROM window while
               opening IDE next time.

8. Add SN8P2212, SN8P2213, SN8P22121 chip function.

9. Revise SN8P2622 PGM_TYPE = 6. 

<Easy Writer PC Software V2.07>

1. Update Easy Writer Driver(*.PRG file) for VPP voltage proposing value
   12.3V ---> 12.7V, and first delay 10ms before VPP12V ON.


<MP Writer PC Software V1.07>

No Change.


<Gang Writer PC Software V1.01>

1. Revise "Read EEPROM" operate interfaces.


<MP-III Writer PC Software V1.00>

1. First issue.


***********************************************************************************************************
        SONiX IDE               	M2IDE_V111      <M2IDE_V111.exe>        (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm111        <M2Asm111.exe>          (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.07
	MP Writer PC Software		V1.07   	<MP_WtV107.exe>
	Gang Writer PC Software		V1.00   	<Gang_WtV100.exe>
	Date: 09/01/2006
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2604A.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617, SN8P2604A.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===========================================================================================================

<B> New Features:

<Assembler M2Asm111>

1. Add SN8P2604A chip function.

2. Bug Fixed : Label name arrange function according to Name or Location is not perfect in the InfoView of IDE.

3. Bug Fixed : Execute PWM function of SN8P2715, PWM does not have wave form to export when FTC0X8 = 1.

4. Bug Fixed : Execute ADC function of SN8P2715, the ADC value(ADB) sometimes is 0xFF, and the LSB 4-bit value
               of 12-bit ADC data is 0.

5. Bug Fixed : Compiling fail when compile the "mov a, #0x87" instruction.

6. Bug Fixed : Execute ADC function of SN8P2708A, the ADC value(ADB) sometimes is 0xFF, and the LSB 4-bit value
               of 12-bit ADC data is 0.

7. Add SN8A2617 LVD code option (LVD_L : 2.0V Reset, LVD_H : 2.4V Reset).


<Easy Writer PC Software V2.07>

No Change.


<MP Writer PC Software V1.07>

1. Add auto-detect function that the MP-Writer must be connected.


<Gang Writer PC Software V1.00>

No Change.


***********************************************************************************************************
        SONiX IDE               	M2IDE_V110      <M2IDE_V110.exe>        (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm110        <M2Asm110.exe>          (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.07
	MP Writer PC Software		V1.06   	<MP_WtV106.exe>
	Gang Writer PC Software		V1.00   	<Gang_WtV100.exe>
	Date: 06/19/2006
***********************************************************************************************************

<A> Supporting Chip:

    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===========================================================================================================

<B> New Features:

<Assembler M2Asm110>

1. Increase the function that can use "extern" to link between files of project.

2. Revise SN8P2624 RAM size as 64 bytes.


<Easy Writer PC Software V2.07>

No Change.


<MP Writer PC Software V1.06>

No Change.


<Gang Writer PC Software V1.00>

No Change.


***********************************************************************************************************
        SONiX IDE               	M2IDE_V109      <M2IDE_V109.exe>        (Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm109        <M2Asm109.exe>          (Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.07
	MP Writer PC Software		V1.06   	<MP_WtV106.exe>
	Gang Writer PC Software		V1.00   	<Gang_WtV100.exe>
	Date: 05/26/2006
***********************************************************************************************************

<A> Supporting Chip:

    Support new chip SN8A2617.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204,  SN8A2617.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===========================================================================================================

<B> New Features:

<Assembler M2Asm109>

1. Bug Fixed : Free run and stopped in breakpoint that setting at Call/Ret instruction, will cause RAM value to be revised.
               Have already revised chip of the question : SN8P2602B, SN8P2613, SN8P2622, SN8P2624,  SN8P2604, SN8P2501B, 
               SN8P2602A, S8KE_TEST, SN8P2715, SN8P2308.

2. Change RFC register of SN8P2308 inc file into RFCM register.

3. In inc file, .Assembly COMMAND increases RBANK_LIMIT item, make compiler only permit to be operated RBANK register by 
   b0xxx instruction.

4. Revise SN8P2501B inc file, when High_Clk of code option chooses IHRC_16M or IHRC_RTC, Fcpu can only choose Fosc/4, Fosc/8,
   or Fosc/16.

5. Support USB to Printer port switching board, PID is 5000.


<Easy Writer PC Software V2.07>

1. Enhance IHRC calibration function in the noise environment.


<MP Writer PC Software V1.06>

1. Support USB to Printer Port switching board, PID is 5000.


<Gang Writer PC Software V1.00>

1. Update USB Gang Writer, PID is 5200.


*******************************************************************************
        SONiX IDE               	M2IDE_V108	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm108	(Only for SN8P2XXX Family)
	Easy Writer PC Software    	V2.06
	MP Writer PC Software		V1.05
	Gang Writer PC Software		V1.00
	Date: 03/10/2006
*******************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2201, SN8P2202, SN8P2203, SN8P2204.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13, SN8P2201, SN8P2202,
    SN8P2203,  SN8P2204.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).
    c. No longer support Writer V3.0 Software.

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm108>

1. Add SN8P2201, SN8P2202, SN8P2203, SN8P2204 chip function.

2. Bug Fixed : Sn8 Report checks check-sum mistake of Sn8 file.

3. In order to improve MP writer programming SN8P2501B IHRC calibration, need to revise PGM_TYPE in inc file
   from "7" to "8".


<Easy Writer PC Software V2.06>

1. Will check VPP while starting the Easy Writer only in revision.

2. Revise SN8P2501B has not execute verify while execute Auto Program.


<MP Writer PC Software V1.05>

No Change.


<Gang Writer PC Software V1.00>

1. First issue.


*******************************************************************************
        SONiX IDE               	M2IDE_V107 	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm107	(Only for SN8P2XXX Family)
	Writer V3.0 PC Software    	V2.07
	Easy Writer PC Software    	V2.06
	MP Writer PC Software  		V1.05
	Date: 12/19/2005
*******************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2501B, SN8P2602B, SN8PC13.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622, SN8P2501B, SN8P2602B, SN8PC13.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm107>

1. Add SN8P2501B, SN8P2602B, SN8PC13 chip function.

2. Bug Fixed : Breaks(Count Break) function of M2IDE that free run after finishing establishing, Breaks unable to stop 
               establishing is clicked.

3. Add Program Type 9 and 11.

4. Remove 32K_X'Tal code option item of SN8P2308, SN8P2622, SN8P2624, SN8P2606, SN8P2608, SN8P2711, SN8P2714, SN8P27142,
   SN8P27143, SN8P2715.

5. Bug Fixed : If Noise filter enable, restrain Fcpu must select being the above Fosc/4 item.

6. Bug Fixed : While SN8P2308 run the T0 RTC mode in the ICE, program into the Green mode will cause T0 interrupt cycle
               is inaccurate.

7. Bug Fixed : The parameter defines with EQU, while reading high byte of the parameter result sometimes can mistake to
               cause.


<Easy Writer PC Software V2.06>

1. Bug Fixed : It causes IDE crash to read and exceed 8K words.

2. Add Program Type 9 and 11.

3. Bug Fixed : Rolling Code count value error.

4. Update .prg file version.


<Writer PC Software V2.07>

1. Add Program Type 9 and 11.

2. Bug Fixed : Rolling Code count value error.


<MP Writer PC Software V1.05>

1. Add Program Type 9 and 11.

2. Bug Fixed : Rolling Code count value error.


*******************************************************************************
        SONiX IDE               	M2IDE_V106 	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm106	(Only for SN8P2XXX Family)
	Writer V3.0 PC Software    	V2.06
	Easy Writer PC Software    	V2.05
	MP Easy Writer PC Software  	V1.04
	Date: 09/27/2005
*******************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2611, SN8P2622.
    Support fully function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A, SN8P2611,  SN8P2622.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).

    SN8P2711 NOTE:
    a. When set EVHENB=1, P4.0 is still ADC input function in emulation, but in real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip will not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm106>

1. Bug fixed : If first instruction is DC define in the assembly file and all of include file
               will cause compile fail.

2. Add SN8P2611, SN8P2622 chip function.

3. Bug fixed : In 4-level stack body of chip 2501, 2602, 2711, 2613, the stack register is 
               3-bit control, so the initial value of STKP bit2 setting 0 will cause stack
               pointer error.

4. Bug Fixed : In the .DATA segment, if the constant defined by EQU is larger than RAM size will
               cause the IDE crash.

5. Add LCD Simulator Function.

6. Bug fixed : In chip SN8P2714/SN8P2715, the RAM value will be modified in the ICE free run mode 
               and execute the RET instruction.

7. SN8P2501A, SN8P2613, SN8P2711 IHRC_16M option of code option must use 16M crystal.

8. Add trace previous single step function.

9. Bug Fixed : P54 of Chip SN8P2308 can't setting pull high resister in input mode.

10. Add debug windows of USB FIFO 0 and USB FIFO 1.

11. Bug Fixed : When setting the slow mode in series SN8P270XA, Fcpu isn't the clock of Fosc devide by 4.

12. Bug Fixed : When compile the chip that support STACK_LIMIT item first and then execute the 
                Easy Writer will cause fail.

13. Bug Fixed : When execute b0bset ftc0x8 instruction in the chip SN8P2714/SN8P2715, the TC0
                will count continually if ICE stop.

14. Bug Fixed : When select code option of High_Clk as IHRC_16M in the chip SN8P2501A, the execute
                frequency will be divided by 2.

15. Bug Fixed : When use the define DB as DB xxxx, if xxxx be defined later, then compiler can show
                the error message that xxxx is undefine.

16. Add the File View of Library files if assembly code has include the *.Lib file.

17. Add Program Type 10.

<Easy Writer PC Software V2.05>

1. Add Program Type 10.

<Writer  PC Software V2.06>

1. Doesn't support the chip that OTP size > 6K(0x1800) words. 

2. Doesn't support the chip that build in 16M RC oscillator except SN8P2501A, such as SN8P2611, SN8P2612,
   SN8P2613, SN8P2711.

3. Add Program Type 10.

<MP-Easy Writer PC Software V1.04>

1. Modify Rolling code function.

2. Add program count function.

3. Add Program Type 10.


*******************************************************************************
        SONiX IDE               	M2IDE_V105 	(Only for SN8ICE 2K)
	Assembler and Debugger  	2Asm105 	(Only for SN8P2XXX Family)
	Writer V3.0 PC Software   	 V2.04
	Easy Writer PC Software    	V2.03
	MP Easy Writer V  V1.02
	Date: 04/25/2005
*******************************************************************************

<A> Supporting Chip:

    Support new chip SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624, SN8P2603A
    It is full function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA, SN8P2711, SN8P2714,
    SN8P27142, SN8P27143, SN8P2715, SN8P2308, SN8P26042, SN8P2612, SN8P2613, SN8P2624,
    SN8P2603A.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE_2K.
    b. SN8IDE V1.99L ~ V1.99Z only support SN8ICE_1K(Alias name is S8KD-2 ICE).

    SN8P2711 NOTE:
    a. P4.0 at EVHENB=1 still ADC input function, but real chip is external reference input.       
    b. P0.0 is with wakeup function in TC0 event counter input mode, but real chip is not.
    c. P0.1 is with wakeup function in TC1 event counter input mode, but real chip is not.
    d. TC0 event counter mode can't be green mode wakeup source, but real chip can. 	
===============================================================================

<B> New Features:

<Assembler M2Asm105>

1. The file be modified will be saved automatically after this file has been compiled.

2. Show the instruction cycle number note in list file.

3. Bug fixed of SN8P2711: 
   a. The instruction cycle time is double if enable watchdog code option.
   b. The ADC result are all 0xFF when ADC's clock source be selected as Fosc.

4. Modification SN8P2501A TC0C register as Read & Modify Write mode.

5. Bug fixed: M2IDE show error message fail cause by wrong error message ID definition.

6. Bug fixed: M2IDE read/write LCD_RAM (bank 15) assign to error bank.

7. Bug fixed: Single step count the cycle value error in all two cycle instruction.

8. Bug fixed: Change ROM code contents manually maybe cause emulation error.

9. Bug fixed: Sometimes the Value title will overlap the Name title in Watch, Reg, All, DS 
   dialog window.

10. Bug fixed: When press the right key of mouse in a blank space of M2IDE Toolbar maybe cause
    the M2IDE crash.

11. Bug fixed: If users set an breakpoint in which instruction to write stack register, this
    instruction will be execute even ICE stop in the breakpoint of this instruction.
    This bug is fixed in all support chip except SN8P2501A.

12. Bug fixed: When M2IDE execute step out function, Assembler can't stop in RET instruction.

 
<Easy Writer PC Software V2.03>

1. Add PGM_TYPE 8.

2. Add SN8 Report function.

3. Modification SN8P2711.prg file

4. Bug fixed: If ICE doesn't be connected to printer port and users load SN8 file will disply
   "No ICE be found error" message. In the mean time if users press any function key will cause
   the Easy Writer driver crash.

5. Bug fixed : Rolling code set more than 13 words can cause rolling code value error, 
               modify can support to 16 words.

<Writer PC Software V2.04>

1. Add PGM_TYPE 8.

2. Bug fixed : Rolling code set more than 13 words can cause rolling code value error, 
               modify can support to 16 words.

<MP-Easy Writer PC Software V1.02>

1. Add PGM_TYPE 8.

2. Bug fixed : Rolling code set more than 13 words can cause rolling code value error, 
               modify can support to 16 words.


*******************************************************************************
        SONiX IDE               	M2IDE_V104 	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm104 	(Only for SN8P2XXX series) 
	Writer V3.0 PC Software    	V2.03
	Easy Writer PC Software    	V2.02
	MP Easy Writer PC Software  	V1.01
	Date: 01/06/2005
*******************************************************************************

<A> Supporting Chip:

    Support new chips: Support SN8P2711, SN8P2714, SN8P2715, SN8P27142 and SN8P27143
      
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE-2K ICE.

    b. SN8IDE V1.99L ~ V1.99Z only support S8KD-2 ICE.

    SN8P2711 NOTE:
    a. In ICE emulation, P4.0 is ADC input function if "EVHENB=1", but in real chip P4.0
       is external reference input. Please refer datasheet for detailed information.

    b. If P0.0 is configured as TC0 event counter input pin. P0.0 has wake-up function in
       ICE Emulation, but there isn't wakeup function in real chip.

    c. If P0.1 is configured as TC1 event counter input pin. P0.1 has wake-up function in
       ICE Emulation, but there isn't wakeup function in real chip.

    d. TC0 event counter overflow can't wakeup chip in green mode, but real chip can.

===============================================================================

<B> New Features:

<Assembler M2Asm104>

1. When ICE reset, show the warning message that ICE just can run lower than 8 MIPS. 

2. Bug fixed: For "B0MOV M,I" instruction, the value of I can't be 0E6h or 0E7h in 
              SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608 and SN8P270XA. If
              I is defined by ROM Label then assembler can't find this limitation.
   E.g.
	Case A:
	B0MOV  Z, #0E6h        ;Assembler can find the limitation
	B0MOV  Z, #0E7h        ;Assembler can find the limitation

	Case B:

	B0MOV Y,#test_table0$M
        B0MOV Z,#test_table0$L ;Assembler can't find the limitation in previous version
        
        B0MOV Y,#test_table1$M
        B0MOV Z,#test_table1$L ;Assembler can't find the limitation in previous version

        ORG 0x0E6
        test_table0:
              dw 0x3412
        ORG 0x0E7
        test_table1:
              dw 0x7856

3. Bug fixed: For "B0XCH A,M" instruction, the address range of M can't be 80h ~ FFh
              in some chips (refer to the new features description of  V1.00).
              If program access the RAM address before this RAM be declared by DS or EQU
              directive then assembler can't detect this "B0XCH A, M" limitation..    

4. Bug fixed: The Auto dialog must be shown RAM value at RAM address 1xxh when Rbank = 1.

5. Bug fixed: Any instruction to write PCL register will cause program counter error
              if the low byte ROM address of this instruction be located at 0xFE or 0xFF.

              Error example:
              
              .CODE
              ORG 0x1FE
              
              MOV A, #0x01     ; ROM address 0x1FE
              B0ADD PCL, A     ; ROM address 0x1FF, PCL be changed will cause error
              JMP   SUB1
              JMP   SUB2

6. Bug fixed: When assembler continuous compile over 512 times will cause open symbol file error.

7. Add RAM bank 15 (for LCD RAM) contents display function. The RAM size of bank 15 be defined
   in device file.


<Easy Writer PC Software V2.02>

No change.
 

<Writer PC Software V2.03 for Writer V3.0 hardware>

No change.


<MP-Easy Writer PC Software V1.01>

No change.



*******************************************************************************
        SONiX IDE               	M2IDE_V103 	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm103 	(Only for SN8P2XXX series) 
	Writer V3.0 PC Software   	 V2.03
	Easy Writer PC Software   	 V2.02
	MP Easy Writer PC Software  	V1.01
	Date: 11/26/2004
*******************************************************************************

<A> Supporting Chip:

    Same as V1.00
    It is full function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE 2K.
    b. SN8IDE V1.99L ~ V1.99Z only support S8KD-2 ICE.

===============================================================================

<B> New Features:

<Assembler M2Asm103>

1. Bug fixed: When stack is full and into the interrupt routine, ICE can't warn stack overflow
              in the interrupt routine.               

2. Bug fixed: When ICE to arise External Reset, Watch dog Reset and LVD Reset, the NT0/NPD
              initial value error. 

               NT0  |  NPD  | ICE                                   | Real Chip
             -------|-------|---------------------------------------|----------------------	
                0   |   0   | Watch dog Reset                       | Watch dog Reset
                    |       | RAM value invariable                  | RAM value invariable
             -------|-------|---------------------------------------|----------------------         
                0   |   1   | Reserved                              | Reserved
             -------|-------|---------------------------------------|----------------------
                1   |   0   | Compile code or to execute Ctrl + F5, | LVD/POR Reset
                    |       | ICE will fill random value into RAM to| RAM unknown
                    |       | simulate real chip status             | 
             -------|-------|---------------------------------------|----------------------  
                1   |   1   | Press ICE external reset key          | External Reset
                    |       | RAM value invariable                  | RAM value invariable


              According to the rules of above table, cancel the Reset Option dialog for select reset type.

3. Bug fixed: When ICE to execute the Download and go function, can't find the correct EV FPGA 
              bit file according to SN8 file if the EV chip has common bit file.

4. Bug fixed: When ICE to execute the single step and happen error, user can't closed IDE program
              and show the "Simulate not stop, do you want to retry." message all the time.

5. Bug fixed: If assembler editor input more than 1024 characters, editor program maybe be closed without any
              warning.

6. Add debug ICE Tool Bar, ex: Step Into(F11), Step Over(F10), Step Out(Shift F11) etc.

7. Bug fixed: Memory rotation instruction of SN8P2501A can't rotates the memory to C flag position.  

8. Bug fixed: SN8P2501A can't setting IO port.

<Easy Writer PC Software V2.02>

1. Bug fixed: If Rolling Code dialog isn't closed by press OK key, the Rolling Code value will be filled '0'.
 
<Writer PC Software V2.03>

1. Add OTP program type 7 for internal use only.

2. Bug fixed: If Rolling Code dialog isn't closed by press OK key, the Rolling Code value will be filled '0'.

3. Bug fixed: Some times, the program or verify fail message doesn't be shown to the dialog window, just be 
              saved into the log file.


<MP-Easy Writer PC Software V1.01>

1. Add OTP program type 7 for internal use only.

2. Bug fixed: If Rolling Code dialog isn't closed by press OK key, the Rolling Code value will be filled '0'.




*******************************************************************************
        SONiX IDE               	M2IDE_V102 	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm102 	(Only for SN8P2XXX series) 
	Writer V3.0 PC Software   	V2.02
	Easy Writer PC Software    	V2.01
	MP Easy Writer PC Software  	V1.0
	Date: 09/20/2004
*******************************************************************************

<A> Supporting Chip:

    Same as V1.00
    It is full function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE 2K.
    b. SN8IDE V1.99L ~ V1.99Z only support S8KD-2 ICE.

===============================================================================

<B> New Features:

<Assembler M2Asm102>

1. Bug fixed: MOVC instruction of SN8P2606, SN8P2608, and SN8P270XA series 
	      will fail in 32KHz crystal and internal low clock.

2. Add .printf, .dbg_cmd, .asm_printf, and .asm_cmd instruction.

3. Add 'Reset Option' item, this option will simulation 'LVD Reset' and 
   'External Reset' in real chip.


<Easy Writer PC Software V2.01>

No change.
 
<Writer PC Software V2.02>

1. Bug fixed: In auto program mode, the verify fail message will not show in dialog.

<MP-Easy Writer PC Software V1.0>

 No change.


*******************************************************************************
        SONiX IDE               	M2IDE_V101 	(Only for SN8ICE 2K)
	Assembler and Debugger 		M2Asm101 	(Only for SN8P2XXX series) 
	Writer V3.0 PC Software    	V2.01
	Easy Writer PC Software    	V2.01
	MP Easy Writer PC Software  	V1.0
	Date: 09/10/2004
*******************************************************************************

<A> Supporting Chip:

    Same as V1.00
    It is full function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE 2K.
    b. SN8IDE V1.99L ~ V1.99Z only support S8KD-2 ICE.

===============================================================================

<B> New Features:

<Assembler M2Asm101>

1. Remove DAA instruction of SN8P2501A and SN8P270XA series.

2. Release ROM address 4 ~ 7 in all SN8P2X series.

3. Remove some no necessary NOP instructions in following built-in macro:
   @RST_WDT, @PWM0_MAX_DUTY, @PWM1_MAX_DUTY

4. Bug fixed: Some times will fail in installation of printer port driver.

5. Bug fixed: In command line mode, some code option combination will cause
              assembly fail.

6. After reset will fill random value into RAM to emulate the contents of real
   chip RAM are random after power on.
   Note: This function is only available at the first time reset after compile
         program.
   

<Easy Writer PC Software V2.01>

 No change.

 
<Writer PC Software V2.01>

 No change.

<MP-Easy Writer PC Software V1.0>

 No change.


*******************************************************************************

        NOTE:
        To avoid users be confused by similar IDE name between SN8ICE 2K (for
        SN8P2X series chip only) and S8KD-2 ICE (for SN8P1X series).        
	SONiX rename the IDE name of "SN8IDE_ICE2K_V2.00" to "M2IDE_V1.00" and
        change the assembler name "S8Asm200_ICE2K" to "M2ASM100"

*******************************************************************************
        SONiX IDE               	M2IDE_V100 	(Only for SN8ICE 2K)
	Assembler and Debugger  	M2Asm100 	(Only for SN8P2XXX series) 
	Writer V3.0 PC Software    	V2.01
	Easy Writer PC Software    	V2.01
	MP Easy Writer PC Software  	V1.0
	Date: 08/10/2004
*******************************************************************************

<A> Supporting Chip:

    The SN8ICE 2K is designed for all SN8P2XXX series chips.
    It is full function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
       
    NOTE:
    a. M2IDE  V1.00 or Later only support SN8ICE 2K.
    b. SN8IDE V1.99L ~ V1.99Z only support S8KD-2 ICE.

===============================================================================

<B> New Features:

<Assembler M2Asm100>

1. Re-enable BTS0 and BTS1 instruction of SN8P270XA.
   Don't use S8Asm200_ICE2K to compile the program of SN8P270XA.

2. Bug fixed: In S8Asm200_ICE2K, sometimes the breakpoint maybe stop at wrong position.

3. Instruction limitations of following chips:
   SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
   
   a. The ROM address 8 of above chips only JMP or NOP instruction is valid.

   b. For "B0MOV M,I" instruction, the value of I can't be 0E6h or 0E7h
      Note: Exclude SN8P2606, SN8P2608
      E.g. "B0MOV  Y, #0E6h" is invalid
           "B0MOV  Y, #00h" is valid

   c. For "B0XCH A,M" instruction, the address range of M can't be 80h ~ FFh 
      Note: 1. 80h ~ FFh is system register area.
            2. Exclude SN8P2606, SN8P2608 
 
   d. Read, modify then write back memory instruction can't access T0C register.
      Note: Exclude SN8P2501A
      E.g. "B0ADD T0C, A" is invalid
           "B0MOV T0C, A" is valid

   e. Remove "DAA" instruction in SN8P2602A and SN8P2604.

4. Show the security checksum in the screen if security code option be enabled.
   The purpose of security checksum is let users compare the OTP writer read back
   checksum (use Read function) if security code option be enabled.

<Easy Writer PC Software V2.01>

1. Doesn't show the VPP voltage in the screen.

2. Modify programming firmware to enhance reliability.

3. Bug fixed: Easy Writer will fail if any debug function have been executed.
 
<Writer PC Software V2.01>

1. Function No change, just change the version to the same as IDE version.

<MP-Easy PC Software V1.0>

1. No change.


*******************************************************************************
        SONiX IDE               	V2.00 	(Only for SN8ICE 2K)
	Assembler and Debugger  	V2.00 	(Only for SN8P2XXX series) 
	Writer V3.0 PC Software   	V2.00
	Easy Writer PC Software   	V2.00
	MP Easy Writer PC Software  	V1.0
	Date: 07/30/2004
*******************************************************************************

<A> Supporting Chip:

    The SN8ICE 2K is designed for all SN8P2XXX series chips.
    It is full function emulation of following chips:
    SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
       
    NOTE:
    a. Version 2.00 or Later only support SN8ICE 2K.
    b. Version 1.99L ~ 1.99Z only support S8KD-2 ICE.

===============================================================================

<B> New Features:

<Assembler V2.00>

1. There is NO NECESSARY to set "ICE_MODE EQU 1" constant and
   includestd "SN8P2X_ICE.H" like 1.99L or later version (1.99L~1.99Z).
   
2. All new friendly user interface including following main features:
   a. Multiple files search function.
   b. View system registers by binary, decimal or hexdecimal format.
   c. View variables by decimal, hexdecimal or ASCII format in memory or watch window.
   d. Window size and location is configurable.
   e. Project window provide two useful sub windows:
      i.  FileView windows: List all files in project for quick open.
      ii. InforView window: Subroutine quick index.
   
3. Instruction limitations of following chips:
   SN8P2501A, SN8P2602A, SN8P2604, SN8P2606, SN8P2608, SN8P270XA.
   
   a. The ROM address 8 of above chips only JMP or NOP instruction is valid.

   b. For "B0MOV M,I" instruction, the value of I can't be 0E6h or 0E7h
      Note: Exclude SN8P2606, SN8P2608
      E.g. "B0MOV  Y, #0E6h" is invalid
           "B0MOV  Y, #00h" is valid

   c. For "B0XCH A,M" instruction, the address range of M can't be 80h ~ FFh 
      Note: 1. 80h ~ FFh is system register area.
            2. Exclude SN8P2606, SN8P2608 
 
   d. Read, modify then write back memory instruction can't access T0C register.
      Note: Exclude SN8P2501A
      E.g. "B0ADD T0C, A" is invalid
           "B0MOV T0C, A" is valid

   e. Remove "DAA" instruction in SN8P2602A and SN8P2604.

   f. SN8P270XA only: Remove BTS0 and BTS1.

4. Install printer port ICE driver automatically.

5. This version doesn't support software simulator.


<Easy Writer PC Software V2.00>
1. First issue for SN8ICE 2K.

2. Always generates log files. The log file will store all operation information
   except read function. The result of read function will be saved in *.BBB file.
   The naming rule of log file as following:
   a. EZMMDDHHmm.log
      MMDDHHmm means current date and time during generate log file.
      (MM: month, DD: day, HH: hour, mm: minute.)
      Restart easy writer program will generate new log file.
   b. Storage directory: The "writer_log" subdirectory of SN8IDE be installed.
      For example: C:\SONIX\Sn8IDE_2.00\writer_log

<Writer PC Software V2.00>
1. First issue for SN8ICE 2K.
2. Always generates log files. The log file will store all operation information
   except read function. The result of read function will be saved in *.BBB file.
   The naming rule of log file as following:
   a. WTMMDDHHmm.log
      MMDDHHmm means current date and time during generate log file.
      (MM: month, DD: day, HH: hour, mm: minute.)
      Restart easy writer program will generate new log file.
   b. Storage directory: The "writer_log" subdirectory of SN8IDE be installed.
      For example: C:\SONIX\Sn8IDE_2.00\writer_log

<MP-Easy Writer PC Software V1.0>
1. First issue.
2. This program can download SN8 file into the EEPROM of MP-Easy Writer by
   printer port.
3. MP-Easy writer is Mass-Production version of Easy writer. Support stand alone
   and rolling code OTP programming.


