#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: £gVision V5.30.0.0
    Copyright (C) 2020 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: erin tseng sonix Flex license: MDK Essential 5.30 (Flex): 12 user(s) (mdk_essential) Support: Jun 2022

    Tool Versions:
    Toolchain:       MDK Essential 5.30 (Flex): 12 user(s)  Version: 5.30.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 6 (build 750)
    Assembler:       Armasm.exe V5.06 update 6 (build 750)
    Linker/Locator:  ArmLink.exe V5.06 update 6 (build 750)
    Library Manager: ArmAr.exe V5.06 update 6 (build 750)
    Hex Converter:   FromElf.exe V5.06 update 6 (build 750)
    CPU DLL:         SARMCM3.DLL V5.30.0.0
    Dialog DLL:      DARMCM1.DLL V1.19.3.0
    Target DLL:      SNLink\SNLINK.dll V1.0.0.2
    Dialog DLL:      TARMCM1.DLL V1.14.2.0

    Project:
    D:\21.Git StarterKit_Package_Release\SN32F790\SN32F790_CMSIS_Firmware_Library_V1.5R\CMSIS Firmware Library_V1.5\Peripheral\SPI\SPI0_Nbytes_Polling\SN32F790_Demo.uvprojx
    Project File Date:  06/21/2022

    Output:
    *** Using Compiler 'V5.06 update 6 (build 750)', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Build target 'SN32F790'
    assembling startup_SN32F790.s...
    compiling PFPA.c...
    compiling SPI0.c...
    compiling main.c...
    compiling system_SN32F790.c...
    compiling Utility.c...
    compiling SPI1.c...
    linking...
    Program Size: Code=1620 RO-data=232 RW-data=4 ZI-data=740
    FromELF: creating hex file...
    After Build - User command #1: HexConvert.exe SN32F790 "D:\21.Git StarterKit_Package_Release\SN32F790\SN32F790_CMSIS_Firmware_Library_V1.5R\CMSIS Firmware Library_V1.5\Peripheral\SPI\SPI0_Nbytes_Polling\obj\SN32F790.HEX"
    INI_Ver = V32
    EXE_Ver = V22
    CheckSum = 0x06B5
    ".\obj\SN32F790.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.5.7.0.pack
                    ARM.CMSIS.5.7.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 5.4.0

    Package Vendor: SONiX
                    http://liveupdate.sonix.com.tw/sonix/develop_tool/MCU/DFP/SONiX.SN32F7_DFP.9.0.4.pack
                    SONiX.SN32F7_DFP.9.0.4
                    SONiX SN32F7 Series Device Support and Examples
       * Component: Startup Version: 1.1.1

    Collection of Component include folders:
      .\RTE\_SN32F790
      C:\Keil_v5\ARM\PACK\ARM\CMSIS\5.7.0\CMSIS\Core\Include
      C:\Keil_v5\ARM\PACK\SONiX\SN32F7_DFP\9.0.4\Device\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:5.4.0

       * Component: SONiX::Device:Startup:1.1.1
          Source file:   Device\Source\ARM\startup_SN32F790.s
          Source file:   Device\Source\system_SN32F790.c
    Build Time Elapsed:  00:00:11