#

##

##

##

##

##

    猩ision Build Log
    Project:
    D:\IC驗證\SN32F280_SN32F780(SU32F90)\Package\SN32F290_Startkit_Package_V0.1R\CMSIS Firmware Library_V1.0\Peripheral\SPI\SPI0_Nbytes_Polling\SN32F290_Demo.uvprojx
    Project File Date:  11/05/2019

    Output:
    Build target 'SN32F290'
    compiling main.c...
    compiling SPI0.c...
    compiling SPI1.c...
    linking...
    Program Size: Code=1580 RO-data=232 RW-data=4 ZI-data=740
    FromELF: creating hex file...
    After Build - User command #1: HexConvert.exe SN32F290 "D:\IC驗證\SN32F280_SN32F780(SU32F90)\Package\SN32F290_Startkit_Package_V0.1R\CMSIS Firmware Library_V1.0\Peripheral\SPI\SPI0_Nbytes_Polling\obj\SN32F290.HEX"
    INI_Ver = V29
    EXE_Ver = V20
    CheckSum = 0xD18C
    ".\obj\SN32F290.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.1.0.pack
                    ARM::CMSIS:CORE:3.30.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 3.30.0

    Package Vendor: SONiX
                    http://liveupdate.sonix.com.tw/sonix/develop_tool/MCU/DFP/SONiX.SN32F2_DFP.1.3.2.pack
                    SONiX::Device:Startup:0.0.1
                    SONiX SN32F2 Series Device Support and Examples
       * Component: Startup Version: 0.0.1

    Collection of Component include folders:
      D:\IC驗證\SN32F280_SN32F780(SU32F90)\Package\SN32F290_Startkit_Package_V0.1R\CMSIS Firmware Library_V1.0\Peripheral\SPI\SPI0_Nbytes_Polling\RTE
      C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.1.0\CMSIS\Include
      C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:3.30.0
          Source file:   CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c

       * Component: SONiX::Device:Startup:0.0.1
          Source file:   Device\Source\ARM\startup_SN32F290.s
          Source file:   Device\Source\system_SN32F290.c

mer */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(61): error: #101: "NDT_IRQn" has already been declared in the current scope NDT_IRQn = 0, /*!< 0 Noise Detection */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(62): error: #101: "USB_IRQn" has already been declared in the current scope USB_IRQn = 1, /*!< 1 USB */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(63): error: #101: "LCD_IRQn" has already been declared in the current scope LCD_IRQn = 2, /*!< 2 LCD Driver */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(64): error: #101: "I2S0_IRQn" has already been declared in the current scope I2S0_IRQn = 3, /*!< 3 I2S0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(65): error: #101: "I2S1_IRQn" has already been declared in the current scope I2S1_IRQn = 4, /*!< 4 I2S1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(66): error: #101: "CMP3_IRQn" has already been declared in the current scope CMP3_IRQn = 5, /*!< 5 CMP3 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(67): error: #101: "SPI0_IRQn" has already been declared in the current scope SPI0_IRQn = 6, /*!< 6 SPI0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(68): error: #101: "SPI1_IRQn" has already been declared in the current scope SPI1_IRQn = 7, /*!< 7 SPI1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(69): error: #101: "UART2_IRQn" has already been declared in the current scope UART2_IRQn = 8, /*!< 8 UART2 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(70): error: #101: "UART3_IRQn" has already been declared in the current scope UART3_IRQn = 9, /*!< 9 UART3 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(71): error: #101: "I2C0_IRQn" has already been declared in the current scope I2C0_IRQn = 10, /*!< 10 I2C0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(72): error: #101: "I2C1_IRQn" has already been declared in the current scope I2C1_IRQn = 11, /*!< 11 I2C1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(73): error: #101: "CMP2_IRQn" has already been declared in the current scope CMP2_IRQn = 12, /*!< 12 CMP2 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(74): error: #101: "UART0_IRQn" has already been declared in the current scope UART0_IRQn = 13, /*!< 13 UART0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(75): error: #101: "UART1_IRQn" has already been declared in the current scope UART1_IRQn = 14, /*!< 14 UART1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(76): error: #101: "CT16B0_IRQn" has already been declared in the current scope CT16B0_IRQn = 15, /*!< 15 16-bit Timer 0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(77): error: #101: "CT16B1_IRQn" has already been declared in the current scope CT16B1_IRQn = 16, /*!< 16 CT16B1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(78): error: #101: "CT16B2_IRQn" has already been declared in the current scope CT16B2_IRQn = 17, /*!< 17 16-bit Timer 2 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(79): error: #101: "CMP1_IRQn" has already been declared in the current scope CMP1_IRQn = 18, /*!< 18 CMP1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(80): error: #101: "CT16B3_IRQn" has already been declared in the current scope CT16B3_IRQn = 19, /*!< 19 16-bit Timer 3 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(81): error: #101: "CT16B4_IRQn" has already been declared in the current scope CT16B4_IRQn = 20, /*!< 20 16-bit Timer 4 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(82): error: #101: "CT16B5_IRQn" has already been declared in the current scope CT16B5_IRQn = 21, /*!< 21 16-bit Timer 5 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(83): error: #101: "EBI_IRQn" has already been declared in the current scope EBI_IRQn = 22, /*!< 22 External Bus Interface */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(84): error: #101: "RTC_IRQn" has already been declared in the current scope RTC_IRQn = 23, /*!< 23 Real-time Clock */ Interface\SPI\SPI1.c: 0 warnings, 30 errors ".\obj\SN32F290.axf" - 30 Error(s), 0 Warning(s).

## Software Packages used:

Package Vendor: ARM http://www.keil.com/pack/ARM.CMSIS.4.1.0.pack ARM::CMSIS:CORE:3.30.0 CMSIS (Cortex Microcontroller Software Interface Standard) * Component: CORE Version: 3.30.0 Package Vendor: SONiX http://liveupdate.sonix.com.tw/sonix/develop_tool/MCU/DFP/SONiX.SN32F2_DFP.1.3.2.pack SONiX::Device:Startup:0.0.1 SONiX SN32F2 Series Device Support and Examples * Component: Startup Version: 0.0.1

## Collection of Component include folders:

D:\IC驗證\SN32F280_SN32F780(SU32F90)\Package\SN32F290_Startkit_Package_V0.1R\CMSIS Firmware Library_V1.0\Peripheral\SPI\SPI0_Nbytes_Polling\RTE C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.1.0\CMSIS\Include C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include

## Collection of Component Files used:

* Component: ARM::CMSIS:CORE:3.30.0 Source file: CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c * Component: SONiX::Device:Startup:0.0.1 Source file: Device\Source\ARM\startup_SN32F290.s Source file: Device\Source\system_SN32F290.c Target not created 8): error: #101: "PendSV_IRQn" has already been declared in the current scope PendSV_IRQn = -2, /*!< -2 Pendable request for system service */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(59): error: #101: "SysTick_IRQn" has already been declared in the current scope SysTick_IRQn = -1, /*!< -1 System Tick Timer */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(61): error: #101: "NDT_IRQn" has already been declared in the current scope NDT_IRQn = 0, /*!< 0 Noise Detection */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(62): error: #101: "USB_IRQn" has already been declared in the current scope USB_IRQn = 1, /*!< 1 USB */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(63): error: #101: "LCD_IRQn" has already been declared in the current scope LCD_IRQn = 2, /*!< 2 LCD Driver */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(64): error: #101: "I2S0_IRQn" has already been declared in the current scope I2S0_IRQn = 3, /*!< 3 I2S0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(65): error: #101: "I2S1_IRQn" has already been declared in the current scope I2S1_IRQn = 4, /*!< 4 I2S1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(66): error: #101: "CMP3_IRQn" has already been declared in the current scope CMP3_IRQn = 5, /*!< 5 CMP3 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(67): error: #101: "SPI0_IRQn" has already been declared in the current scope SPI0_IRQn = 6, /*!< 6 SPI0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(68): error: #101: "SPI1_IRQn" has already been declared in the current scope SPI1_IRQn = 7, /*!< 7 SPI1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(69): error: #101: "UART2_IRQn" has already been declared in the current scope UART2_IRQn = 8, /*!< 8 UART2 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(70): error: #101: "UART3_IRQn" has already been declared in the current scope UART3_IRQn = 9, /*!< 9 UART3 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(71): error: #101: "I2C0_IRQn" has already been declared in the current scope I2C0_IRQn = 10, /*!< 10 I2C0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(72): error: #101: "I2C1_IRQn" has already been declared in the current scope I2C1_IRQn = 11, /*!< 11 I2C1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(73): error: #101: "CMP2_IRQn" has already been declared in the current scope CMP2_IRQn = 12, /*!< 12 CMP2 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(74): error: #101: "UART0_IRQn" has already been declared in the current scope UART0_IRQn = 13, /*!< 13 UART0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(75): error: #101: "UART1_IRQn" has already been declared in the current scope UART1_IRQn = 14, /*!< 14 UART1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(76): error: #101: "CT16B0_IRQn" has already been declared in the current scope CT16B0_IRQn = 15, /*!< 15 16-bit Timer 0 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(77): error: #101: "CT16B1_IRQn" has already been declared in the current scope CT16B1_IRQn = 16, /*!< 16 CT16B1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(78): error: #101: "CT16B2_IRQn" has already been declared in the current scope CT16B2_IRQn = 17, /*!< 17 16-bit Timer 2 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(79): error: #101: "CMP1_IRQn" has already been declared in the current scope CMP1_IRQn = 18, /*!< 18 CMP1 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(80): error: #101: "CT16B3_IRQn" has already been declared in the current scope CT16B3_IRQn = 19, /*!< 19 16-bit Timer 3 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(81): error: #101: "CT16B4_IRQn" has already been declared in the current scope CT16B4_IRQn = 20, /*!< 20 16-bit Timer 4 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(82): error: #101: "CT16B5_IRQn" has already been declared in the current scope CT16B5_IRQn = 21, /*!< 21 16-bit Timer 5 */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(83): error: #101: "EBI_IRQn" has already been declared in the current scope EBI_IRQn = 22, /*!< 22 External Bus Interface */ C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include\SN32F290.h(84): error: #101: "RTC_IRQn" has already been declared in the current scope RTC_IRQn = 23, /*!< 23 Real-time Clock */ Interface\SPI\SPI1.c: 0 warnings, 30 errors compiling Utility.c... assembling startup_SN32F290.s... compiling system_SN32F290.c... ".\obj\SN32F290.axf" - 60 Error(s), 0 Warning(s).

## Software Packages used:

Package Vendor: ARM http://www.keil.com/pack/ARM.CMSIS.4.1.0.pack ARM::CMSIS:CORE:3.30.0 CMSIS (Cortex Microcontroller Software Interface Standard) * Component: CORE Version: 3.30.0 Package Vendor: SONiX http://liveupdate.sonix.com.tw/sonix/develop_tool/MCU/DFP/SONiX.SN32F2_DFP.1.3.2.pack SONiX::Device:Startup:0.0.1 SONiX SN32F2 Series Device Support and Examples * Component: Startup Version: 0.0.1

## Collection of Component include folders:

D:\IC驗證\SN32F280_SN32F780(SU32F90)\Package\SN32F290_Startkit_Package_V0.1R\CMSIS Firmware Library_V1.0\Peripheral\SPI\SPI0_Nbytes_Polling\RTE C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.1.0\CMSIS\Include C:\Keil_v5\ARM\PACK\SONiX\SN32F2_DFP\1.3.2\Device\Include

## Collection of Component Files used:

* Component: ARM::CMSIS:CORE:3.30.0 Source file: CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c * Component: SONiX::Device:Startup:0.0.1 Source file: Device\Source\ARM\startup_SN32F290.s Source file: Device\Source\system_SN32F290.c Target not created rCodeTemplates\ARM\ITM_Retarget.c * Component: SONiX::Device:Startup:0.0.1 Source file: Device\Source\system_SN32F280.c Source file: Device\Source\ARM\startup_SN32F280.s Target not created