#

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: £gVision V5.30.0.0
    Copyright (C) 2020 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: edan chen, sonix, LIC=HN9ML-X8YP2-GHH27-CI9YR-AGZ8Y-P21MQ

    Tool Versions:
    Toolchain:       PK51 Prof. Developers Kit: 6 user  Version: 9.54
    Toolchain Path:  C:\Keil_v5\C51\BIN
    C Compiler:      C51.exe V9.54
    Assembler:       A51.exe V8.02c
    Linker/Locator:  LX51.exe V4.66.41.0
    Library Manager: LIBX51.exe V4.30.1.0
    Hex Converter:   OHX51.exe V1.45.0.0
    CPU DLL:         S8051.DLL V3.100.0.0
    Dialog DLL:      DCore51.DLL V2.81.4.0
    Target DLL:      SNLINK\SNLINK.dll V1, 0, 0, 4
    Dialog DLL:      TCore51.DLL V2.66.2.1

    Project:
    D:\1. IC\SH56E40A(SN8F5754)\16. Lib Package\5. Peripheral Demo Code\5754 Demo Code\14. SN8F5754_UART\TX Polling_RX Interrupt\4. UART0_Mode1 with CRC\UART Mode1.uvproj
    Project File Date:  02/09/2022

    Output:
    Rebuild target 'UART'
    compiling main.c...
    assembling OPTIONS_SN8F5754.A51...
    assembling STARTUP.A51...
    compiling uart0.c...
    compiling uart1.c...
    compiling crc.c...
    linking...
    Program Size: data=58.0 xdata=68 const=0 code=993
    creating hex file from ".\Objects\SN8F5754_UART"...
    User command #1: HexConvert.exe SN8F5754 "D:\1. IC\SH56E40A(SN8F5754)\16. Lib Package\5. Peripheral Demo Code\5754 Demo Code\14. SN8F5754_UART\TX Polling_RX Interrupt\4. UART0_Mode1 with CRC\Objects\SN8F5754_UART.HEX"
    INI_Ver = V31
    EXE_Ver = V21
    CheckSum = 0x9F3E
    ".\Objects\SN8F5754_UART" - 0 Error(s), 0 Warning(s).
    Build Time Elapsed:  00:00:02