#

##

##

##

##

##

    µVision Build Log
    Project:
    D:\MCU\ST32F90\Release\SN32F760_Startkit_Package_V2.1\CMSIS Firmware Library_V2.1\PMU\DeepSleep\SN32F760_Demo.uvprojx
    Project File Date:  05/18/2015

    Output:
    Rebuild target 'SN32F760'
    compiling main.c...
    compiling PFPA.c...
    compiling PMU_drive.c...
    compiling Utility.c...
    compiling GPIO.c...
    assembling startup_SN32F760.s...
    compiling system_SN32F760.c...
    linking...
    Program Size: Code=4448 RO-data=232 RW-data=8 ZI-data=608
    FromELF: creating hex file...
    After Build - User command #1: HexConvert.exe SN32F760 "D:\MCU\ST32F90\Release\SN32F760_Startkit_Package_V2.1\CMSIS Firmware Library_V2.1\PMU\DeepSleep\obj\SN32F760.HEX"
    HexConvertVer = V02
    CheckSum = 0xBF2C
    ".\obj\SN32F760.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.1.0.pack
                    ARM::CMSIS:CORE:3.30.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 3.30.0

    Package Vendor: SONiX
                    http://liveupdate.sonix.com.tw/sonix/develop_tool/MCU/DFP/SONiX.SN32F7_DFP.1.1.1.pack
                    SONiX::Device:Startup:1.1.0
                    SONiX SN32F7 Series Device Support and Examples
       * Component: Startup Version: 1.1.0

    Collection of Component include folders:
      D:\MCU\ST32F90\Release\SN32F760_Startkit_Package_V2.1\CMSIS Firmware Library_V2.1\PMU\DeepSleep\RTE
      C:\Keil\ARM\PACK\ARM\CMSIS\4.1.0\CMSIS\Include
      C:\Keil\ARM\PACK\SONiX\SN32F7_DFP\1.1.1\Device\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:3.30.0
          Source file:   CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c

       * Component: SONiX::Device:Startup:1.1.0
          Source file:   Device\Source\ARM\startup_SN32F760.s
          Source file:   Device\Source\system_SN32F760.c